****

**KASHKAVAL - CURD PROCESSİNG TANK**

**“ 1000 liter capacity. Vertical model**

**“ Manufactured from AISI 304 qualıty staınless steel. 1. body 2.5 mm,2. body 2,5 mm and isolated body**

**is 1.5 mm aısı 304 quality stainless steel. Insulation range is 50 mm with polyurethane without cfc.**

**“ Platform with stainless steel. It has electricity damper. Works with electricity**

**“ Its mixer has speed control**

**“ Heatıng with 380 volt electrical resistances**

**“ Product output ıs DN 100 staınless steel valve**

**“Digital temperature display and control mechanism in the control panel**

**KASHKAVAL INFİLTRATİON AND CHEESE WATER STOCK SHIP**

**“ Manufactured from AISI 304 stainless steel.**

**“ 1000 liter capacity**

**“ Two pieces nested. Rotating wheels are available in stainless steel**

**“ DN 40 staınless steel valve**

**SANTRİFÜJ POMPA**

**“Manufactured from AISI 304 stainless steel.**

**“Sheathed in stainless.**

**Cheese cutters- PROCESSED KASHKAVAL PRODUCTİON LİNE (With Water)**

**“ Manufactured from AISI 304 stainless steel.**

**“ Equipment have electric engines. Cheese don’t to adhesion of through special design.**

**“ Equipment are  heated with hot water**

**“ Digital temperature display and control mechanism in the control panel**

**CHEESE TABLE**

**“Manufactured from AISI 304 stainless steel. 2 shelves**

**KASHKAVAL TROLLEY**

**“ Manufactured from AISI 304 stainless steel**

**“4 shelves AND 4 rotating wheels are available in stainless steel**

**VACUUM MACHİNE**

**“ Manufactured from AISI 304 stainless steel.**

**“ Portable model.**

**CURD HANGER WİTH BOAT**

**“ Manufactured from AISI 304 stainless steel.**

**“ There is the boat of under for curd water.**

**REFRİGERATOR**

**“ 345 liter volüme**